22323 bytes read
    block 1: crc = 0xA212ABF8, combined CRC = 0xA212ABF8, size = 22373
    too repetitive; using fallback sorting algorithm
      22373 in block, 13504 after MTF & 1-2 coding, 79+2 syms in use
      pass 1: size is 17143, grp uses are 38 62 2 92 6 71 
      pass 2: size is 6506, grp uses are 28 71 0 86 9 77 
      pass 3: size is 6479, grp uses are 26 70 0 81 11 83 
      pass 4: size is 6469, grp uses are 26 69 0 74 17 85 
      bytes: mapping 19, selectors 66, code lengths 134, codes 6465
    final combined CRC = 0xA212ABF8
   6710 after compression
bit 0   -5  DATA_ERROR_MAGIC 
bit 1   -5  DATA_ERROR_MAGIC 
bit 2   -5  DATA_ERROR_MAGIC 
bit 3   -5  DATA_ERROR_MAGIC 
bit 4   -5  DATA_ERROR_MAGIC 
bit 5   -5  DATA_ERROR_MAGIC 
bit 6   -5  DATA_ERROR_MAGIC 
bit 7   -5  DATA_ERROR_MAGIC 
bit 8   -5  DATA_ERROR_MAGIC 
bit 9   -5  DATA_ERROR_MAGIC 
bit 10   -5  DATA_ERROR_MAGIC 
bit 11   -5  DATA_ERROR_MAGIC 
bit 12   -5  DATA_ERROR_MAGIC 
bit 13   -5  DATA_ERROR_MAGIC 
bit 14   -5  DATA_ERROR_MAGIC 
bit 15   -5  DATA_ERROR_MAGIC 
bit 16   -5  DATA_ERROR_MAGIC 
bit 17   -5  DATA_ERROR_MAGIC 
bit 18   -5  DATA_ERROR_MAGIC 
bit 19   -5  DATA_ERROR_MAGIC 
bit 20   -5  DATA_ERROR_MAGIC 
bit 21   -5  DATA_ERROR_MAGIC 
bit 22   -5  DATA_ERROR_MAGIC 
bit 23   -5  DATA_ERROR_MAGIC 
bit 24   0  OK really ok!
bit 25   -5  DATA_ERROR_MAGIC 
bit 26   -5  DATA_ERROR_MAGIC 
bit 27   0  OK really ok!
bit 28   -5  DATA_ERROR_MAGIC 
bit 29   -5  DATA_ERROR_MAGIC 
bit 30   -5  DATA_ERROR_MAGIC 
bit 31   -5  DATA_ERROR_MAGIC 
bit 32   -4  DATA_ERROR 
bit 33   -4  DATA_ERROR 
bit 34   -4  DATA_ERROR 
bit 35   -4  DATA_ERROR 
bit 2412   -4  DATA_ERROR 
bit 4789   -4  DATA_ERROR 
bit 7166   -4  DATA_ERROR 
bit 9543   -4  DATA_ERROR 
bit 11920   -4  DATA_ERROR 
bit 14297   -4  DATA_ERROR 
bit 16674   -4  DATA_ERROR 
bit 19051   -4  DATA_ERROR 
bit 21428   -4  DATA_ERROR 
bit 23805   -4  DATA_ERROR 
bit 26182   -4  DATA_ERROR 
bit 28559   -4  DATA_ERROR 
bit 30936   -4  DATA_ERROR 
bit 33313   -4  DATA_ERROR 
bit 35690   -4  DATA_ERROR 
bit 38067   -4  DATA_ERROR 
bit 40444   -4  DATA_ERROR 
bit 42821   -4  DATA_ERROR 
bit 45198   -4  DATA_ERROR 
bit 47575   -4  DATA_ERROR 
bit 49952   -4  DATA_ERROR 
bit 52329   -4  DATA_ERROR 
all ok
