# test that gdbserver/gdb properly handle a PIC executable
# On linux, this implies a proper transfer of the auxv
# information via the gdbserver protocol packet qXfer:auxv:read:
# The content of the auxv data can be shown by gdb using
# gdb command 'info auxv'
prereq: test -e gdb.pic
prog: main_pic
vgopts: --tool=memcheck --vgdb=yes --vgdb-error=0 --vgdb-prefix=./vgdb-prefix-mcmain_pic
stdout_filter: filter_gdb
stderr_filter: filter_memcheck_monitor
progB: gdb
argsB: --quiet -l 60 --nx ./main_pic
stdinB: mcmain_pic.stdinB.gdb
stdoutB_filter: filter_gdb
stderrB_filter: filter_memcheck_monitor

