# test the signal handling, when signals are *not* passed to the Valgrind guest.
# We detect this two ways:
#   the gdb output will not contain the signal handling
#   faultstatus C code will report a failure for the signal not passed
#      (i.e. SIGBUG, Test 3). Other tests will be succesful, because signals
#      are eventually passed.
prereq: test -e gdb
prog: ../none/tests/faultstatus
vgopts: --tool=memcheck --vgdb=full --vex-iropt-register-updates=allregs-at-mem-access --vgdb-error=0 --vgdb-prefix=./vgdb-prefix-mcsignopass
stderr_filter: filter_memcheck_monitor
stderr_filter_args: faultstatus.c
progB: gdb
argsB: --quiet -l 60 --nx ../none/tests/faultstatus
stdinB: mcsignopass.stdinB.gdb
stdoutB_filter: filter_gdb
stderrB_filter: filter_make_empty

