Signal        Stop	Print	Pass to program	Description
SIGSEGV       Yes	Yes	No		Segmentation fault
Signal        Stop	Print	Pass to program	Description
SIGBUS        Yes	Yes	Yes		Bus error
Signal        Stop	Print	Pass to program	Description
SIGFPE        Yes	Yes	Yes		Arithmetic exception
Continuing.
Program received signal SIGSEGV, Segmentation fault.
0x........ in test1 () at faultstatus.c:105
105		*BADADDR = 'x';
Continuing.
Program received signal SIGSEGV, Segmentation fault.
0x........ in test1 () at faultstatus.c:105
105		*BADADDR = 'x';
Continuing.
Program received signal SIGSEGV, Segmentation fault.
0x........ in test1 () at faultstatus.c:105
105		*BADADDR = 'x';
Continuing.
Program received signal SIGSEGV, Segmentation fault.
0x........ in test1 () at faultstatus.c:105
105		*BADADDR = 'x';
Continuing.
Program received signal SIGSEGV, Segmentation fault.
0x........ in test1 () at faultstatus.c:105
105		*BADADDR = 'x';
Continuing.
Program received signal SIGSEGV, Segmentation fault.
0x........ in test1 () at faultstatus.c:105
105		*BADADDR = 'x';
Continuing.
Program received signal SIGSEGV, Segmentation fault.
0x........ in test1 () at faultstatus.c:105
105		*BADADDR = 'x';
Continuing.
Program received signal SIGSEGV, Segmentation fault.
0x........ in test1 () at faultstatus.c:105
105		*BADADDR = 'x';
Continuing.
Program received signal SIGSEGV, Segmentation fault.
0x........ in test1 () at faultstatus.c:105
105		*BADADDR = 'x';
Continuing.
Program received signal SIGSEGV, Segmentation fault.
0x........ in test1 () at faultstatus.c:105
105		*BADADDR = 'x';
Continuing.
Program received signal SIGSEGV, Segmentation fault.
0x........ in test1 () at faultstatus.c:105
105		*BADADDR = 'x';
Signal        Stop	Print	Pass to program	Description
SIGSEGV       No	Yes	Yes		Segmentation fault
Continuing.
Program received signal SIGSEGV, Segmentation fault.
Program received signal SIGBUS, Bus error.
0x........ in test3 () at faultstatus.c:115
115		mapping[FILESIZE+10];
Continuing.
Program received signal SIGFPE, Arithmetic exception.
